Typical Gas engine spreader wiring most models.

Note before permanently mounting the receiver.   
  
locate the receiver on the drivers side of the spreader outside the engine compartment. Test the unit from the cab of your vehicle to ensure operation before permanently mounting the unit. Use rubber washers if bolting the unit down.

**From Wireless To Spreader**

Green wire Brown Throttle down(throttle control)

Blue wire Red throttle up and choke (throttle control)

Orange wire Black wire from magneto – kill switch

Black Wire goes to battery ground

Red wire use fuse link goes to Battery hot

Yellow wire goes to black wire of relay socket

Brown wire goes to small post of starter solenoid

Note other small post of solenoid is typically going to ground

**Wires from Relay socket Connects to**

Yellow clutch wire

White ground

Black wireless receiver Yellow wire

Blue 12 volt power

Red (center wire) (not used) this is 12 volt constant power)

It is very important that when the unit is not in use that the power is disconnected

